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Specification Text

Automatic Sliding Door

Dimensions

Overall width

........... mm

Overall height

........... mm

Passage width

........... mm (700 – 3000 mm)

Passage height

........... mm

TORMAX iMotion® 2302 Sliding Door Drive 

Automatic sliding door drive for single or double-leaf sliding doors, standard or telescopic

· Door leaf weight 2 x 180 kg, 1 x 200 kg

· Cross section header profile (H x D) 150 x 166 mm
· In compliance with current guidelines  2006/42/EG, 2006/95/E, 2004/108/EG
· In compliance with current standards DIN 18650, EN 16005, EN 60335-1,-2-103, 
EN 61000-6-2,-3, EN ISO 13849-1:2008, Performance level „d“
· Approvals: CE incl. RoHS, TÜV
( _ )
Electromechanical sliding door drive with wear-free synchronous motor technology and programmable processor control. Gearless, brushless low-maintenance AC motor. Mains supply 115 VAC/60 Hz or 230 VAC/50 Hz

· Protective system IP22, ambient temperature, –20 °C to +50 °C. 

· Double rollers with groove for ideal load distribution and smooth directional stability

· Adjustable counter roller for low friction operation free from play 

· Positive fit design with a securely retained trolley.

· Easily replaceable noise-damped guide rail.

· Mounting method: Lintel mounting, wall mounting, ceiling mounting.

Control System
· 32 Bit/30 MHz processor for high performance.

· 8 inputs (4 testable safety devices)

· 3 programmable outputs (optional feedback signals for different door statuses, such as: Closed, Open, Fault, Lock status, Light pulse, Gong pulse).

· Modular extendable by max. 2 I/O-modules (4 in-/outputs each)

· Interfaces: LIN BUS, CAN BUS, RS 232

· Automatic detection of system-specific data for optimal motion control, permanent operating diagnosis.

· Fault recognition, display and log.

· Multifunctional user interface with selectable operating modes: OFF, AUTOMATIC 1, AUTOMATIC 2, EXIT, OPEN and MANUAL. 
Detailed status and fault diagnosis. Freewheeling function and reset selectable on operating unit. 
· Electronic obstacle recognition in closing and opening directions, adjustable reversing sensibility.

· Easy-to-move manual operation in the event of a power failure; also available with automatic speed limitation as an option.
· Emergency opening for autonomous door opening in the event of power failure in the unlocked state.
· Many programmable functions such as operating modes, feed-back, special functions, air-lock/ porch function etc.
· Integration in higher-level system possible, e.g. a building management system, optionally via potential-free contacts or a bus system.

Door leaves

( _ )
Sliding leaf

( _ )
Stationary lateral components

( _ )
Stationary fanlights, ( _ ) -part

Profiles

( _ )
TORMAX Profile System LR 12

Single-sheet glazing ESG, VSG, wet

Glazing thickness 6 – 12 mm

Type of glazing: wet, single-sheet/compound toughened safety glass

Facial width 22 mm, base height 80 mm, profile depth 20 mm

( _ )
TORMAX Profile System LR 22B

Single-sheet or insulating glazing, dry

Glass thickness dry 8.5 – 10 mm, 21.5 – 23 mm, wet 6 – 28 mm

Facial width 30 mm, base height 78 mm, profile depth 34 mm

( _ )
TORMAX Profile System LR 32THERM


Insulating glazing, wet


Glazing thickness max. 32mm,


Facial width 35mm, base height 85mm, profile depth 40mm

( _ )
Make………… 

Floor guide

( _ )
Surface-mounted floor guide

( _ )
Continuous floor guide in CNS, including glider in the sliding leaf

( _ )
Continuous floor guide in aluminium anodised E6/EV1 incl. gliding piece in sliding leaf

Colour of visible profiles

Elox anodising colour
…………….

Powder coating RAL
…………….

…………….…………….………………..

Glazing

( _ )
Single-sheet safety glass 10 mm, heat soak tested

( _ )
Compound safety glass 10 mm, with 0.78 mm film 

( _ )
Insulating glass comprising 2 x 5 mm single-sheet safety glass, heat soak tested, 22 mm 

Overall thickness, Ug 1.3 W/m2K

( _ )
Insulating glass comprising 2 x 6 mm compound safety glass, film 0.78 mm, 22 mm

Overall thickness, Ug 1.3 W/m2K

( _ )
Double insulating glass comprising 2 x VSG, overall thickness 31.1mm, Ug 1.0W/(m2/K)

( _ )
Triple insulating glass comprising 3 x ESG, overall thickness 32mm, Ug 0.8W/(m2/K)
( _ )
Make………… 

Sensors

Activation

( _ )
Radar

( _ )
Active infrared

( _ )
Passive infrared

( _ )
Contact-free hand switch

( _ )
Manual hand switch

Safety facility

( _ )
Dynamic safety (with/without testing)

( _ )
Static safety (with/without testing)

( _ )
Combined detector/alarm (radar and 3D protective light curtain AIR) with testing


Safety assessment conforming to DIN 18650 / EN 16005 recommended. Within the scope of the guidelines for machines 2006/42/EG a declaration of conformity for the door installation is mandatory.

Accessories

( _ )
User interface with 6 operating modes and fault display, 45 x 45 mm. Can be installed laterally in the drive cover or externally for installation on the wall or concealed installation in the wall. Suitable for Legrand system.

( _ )
3-position operating mode switch mounted in plastic case
( _ )
Monitored battery module for emergency power supply

( _ )
Electromechanical lock (bistable lock) with feedback, acting only on hardened holding bolts of the leaf, not acting on the toothed belt or deflection pulley

( _ )
Emergency opening including burglary protected emergency unlocking

( _ )
Emergency opening monitoring facility

( _ )
Emergency OFF switch, optionally surface-mounted or flush-mounted, 
with glass cover and frame

( _ )
Integration in system network with contacts communication

( _ )
Integration in system network with bus communication
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