{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Introduction","Manufacturer_overview","Product_information"],"not_rendered":{"charts":0,"images":4,"macros":0,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Introduction","index":0,"n_rows":32,"n_cols":15,"rows_kept":32,"cut":false,"hidden":false,"merged":[[24,2,24,17],[25,2,25,17],[42,3,44,6],[13,1,13,17],[14,1,14,17],[17,1,17,17],[18,1,18,17],[21,1,21,17],[23,2,23,17],[1,9,2,12],[1,14,2,17],[5,13,6,15],[8,1,8,17],[9,1,9,17],[10,1,10,17]]}
[]
[{"$nulls":9},"Add overview information »",{"$nulls":4},"Add product information »"]
[]
[]
[]
[]
[null,"Manufacturer Product Data Template"]
[]
[null,"This is a Manufacturer Product Data Template for Paving laying course mortars."]
[]
[null,"1. Purpose"]
[]
[]
[null,"The growth of BIM has increased the requirement for data to be shared in a consistent format. The Product Data Templates are electronic spreadsheets which you can complete to provide construction professionals with the product data and structured technical information they need for Level 2 BIM projects.  By publishing information about your products in this standardised and structured format your product information will be compatible with the UK’s Level 2 BIM requirements.   \n\nOnce you have completed the template you can host it on your own website or distribute it to your customers.  The template is your first step in making your product data fit for Level 2 BIM.\n"]
[null,"2. Description"]
[]
[]
[null,"Use this Product Data Template to create a set of technical information for your Paving laying course mortars in a standard format which aligns with UK Level 2 BIM terminology.  The template contains a set of fields which cover all the information that is required about your product, and is pre-populated with the relevant Uniclass2015 and NBS classification codes."]
[null,"3. Further support from NBS"]
[]
[]
[null,"NBS provides unique opportunities for manufacturers to place digital information about your products and services directly in front of designers and other construction professionals at the right time and in the right format.  Contact us today to discuss how we can help your business.  Our services include:"]
[]
[null,null,"1. NBS National BIM Library\nThe award-winning free to use library of generic and manufacturer BIM objects.  Manufacturers can either choose the NBS BIM experts to author and host your BIM objects on nationalBIMlibrary.com, or you can create your own objects to meet the trusted NBS BIM Object Standard and we will host them on the website.  All BIM objects hosted on the NBS National BIM Library are displayed within the BIM Toolkit at the design stage of a project.  "]
[null,null,"2. NBS Plus\nNBS Plus is a dedicated section within NBS software for manufacturers’ technical product information.  This is embedded into relevant specification clauses within NBS software which means that designers can instantly add your products into their project specification.  Product specifications from NBS Plus are also shown within the BIM Toolkit at the specification stage of a Level 2 BIM project."]
[null,null,"3. RIBA Product Selector\nA free online resource and the industry-leading index of manufacturers’ product information in the UK. Ensure your company profile, products, catalogues and case studies are available on ribaproductselector.com to increase your online brand recognition and reach. Technical literature from ribaproductselector.com is also included within the NBS BIM Toolkit, providing additional exposure within the Level 2 BIM environment."]
[]
[null,"Contact us now for further information:"]
[]
[null,"Telephone",null,"+44 (0)345 200 1056"]
[null,"Email",null,"info@riba-insight.com"]
[null,"Website",null,"www.riba-insight.com"]

{"sheet":"Manufacturer_overview","index":1,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[11,0,11,1],[12,0,12,1]]}
["Paving "," permeable laying course aggregate"]
[]
["Name","tuffgrit  permeable laying course aggregate",null,"Manufacturer","SteinTec by tuffbau Ltd."]
["Description","Paving laying course aggreagtes are described by characteristics such as delivery condition, mortar designation and characteristics.\nAn example use may be within a small unit paving overlay system.",null,"Address line 1","1 Nofrthwick Road"]
["Version","2",null,"Address line 2","Canvey Island"]
[null,null,null,"Address line 3","Essex"]
["Classification",null,null,"Postcode","SS8 0PU"]
["Uniclass2015","Pr_20-31-04-62 Permeable Laying Course Aggregates",null,"Telephone","01708 860049"]
["NBS Code","45-55-50/335 Permeable Laying Course Aggregates",null,"Fax","01708 860893"]
["NRM1","-",null,"Website","www.tuffbau.com"]
[null,null,null,"Email","info@tuffbau.com"]

{"sheet":"Product_information","index":2,"n_rows":8,"n_cols":40,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[null,"2","4","4","4","4","4","4","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6","6"]
["Reference","Description","Manufacturer","Standard","Delivery condition","Mortar designation","Characteristics","Moisture content","Asset type","ModelNumber","Warranty guarantor (parts)","Warranty duration (parts)","Warranty guarantor (labour)","Warranty duration (labour)","Warranty duration unit","Replacement cost","Expected life","Duration unit","Warranty description","Nominal length","Nominal width","Nominal height","ModelReference","Shape","Size","Colour","Finish","Grade","Material","Constituents","Features","Accessibility performance","Sustainability performance","Code performance","Serial number","Installation date","Warranty start date","Tag number","Bar code","Asset identifier"]
["ModelReference","Description","Manufacturer","Standard","DeliveryCondition","MortarDesignation","Characteristics","MoistureContent","AssetType","ModelNumber","WarrantyGuarantorParts","WarrantyDurationParts","WarrantyGuarantorLabor","WarrantyDurationLabor","WarrantyDurationUnit","ReplacementCost","ExpectedLife","DurationUnit","WarrantyDescription","NominalLength","NominalWidth","NominalHeight","ModelReference","Shape","Size","Color","Finish","Grade","Material","Constituents","Features","AccessibilityPerformance","SustainabilityPerformance","CodePerformance","SerialNumber","InstallationDate","WarrantyStartDate","TagNumber","BarCode","AssetIdentifier"]
["A reference for the system or product","A description of the type of object to detail any design intent.","The Manufacturer of the Paving laying course mortars.","An example value being To BS 7533-7 paragraph 5.1.2.","An example value being Bagged.","An example value being Type A.","An example value being As BS 7533-7 Table C.4.","An example value being Moist mix.","An indication of whether the object is fixed or movable.","The product, item or unit number assigned by the manufacturer of the object.","Email address for the organisation responsible for the parts warranty.","Duration of parts warranty.","Email address for the organisation responsible for the labour warranty.","Duration of labour warranty.","Duration of warranties (typical value is 'years').","An indicative cost for unit replacement.","The typical service life of the object.","Duration of expected life (typical value is 'years')","Description of the warranty content and any exclusions.","Typically the larger or primary horizontal dimension.","Nominal width of product, typically the characteristic or secondary horizontal or characteristic dimension.","Typically the vertical or secondary characteristic dimension.","The name of the object as used by the manufacturer.","Characteristic shape of product.","Characteristic size of product.","Characteristic or primary colour of product.","Characteristic or primary finish of product.","Standard grading which the product corresponds.","Characteristic or primary material of product.","Optional constituent features, parts or finishes.","Other important characteristics or features relevant to product specification.","The accessibility issue(s) which the object satisfies.","Description of the sustainability issue(s) which the object satisfies","The code compliance requirement(s) which the object satisfies","The serial number assigned to an occurrence of a product by the manufacturer (per instance).","The date that the manufactured item was installed (per instance).","The date on which the warranty commences.","The tag number assigned to an occurrence of a product by the occupier (per instance).","The identity of the bar code (or rfid) given to an occurrence of the product (per instance).","The identification assigned to an asset that enables its differentiation from other assets."]
["SteinTec tuffgrit aggregate blend.","Carefully blended water permeable crushed igneous rock aggregate  suitable for bedding in modular bound or unbound pavement construction employing natural stone setts and slabs or pre-cast concrete blocks and flags","SteinTec by tuffbau Ltd","BS 7533-13:2009","Bagged dry or bulk.","NA","Uncompacted bulk density;1.553 tonnes/m3. Compacted bulk density ; 1.733 tonnes/m3. Conforms with BS7533-13 table A2. Accords with : EN13242 Grading Gc85-15. Crushed particle index C90/3. Shape index Sl20, Flakiness index Fl14. Abrasion coefficient LA20, Resisitance to wear Mde15. Water absorption WA24 1.","NA","Fixed","SteinTec tuffgrit aggregate blend.","info@tuffbau.com","6 months","NA","NA","NA","NA",">40 years",">40 years","tuffbau Ltd warrants that the bagged product components will meet the specified performance criteria at production","0.00mm","0.00mm","0.00mm","SteinTec tuffgrit aggregate blend","formless","NA","NA","NA","NA","Water permeable crushed igneous rock aggregate.","NA","Frost resistant, Resistant to De-Icing Salts. Impact resistant, non shrinking, Free-flowing permeable, outstanding thermal and dynamic performance.","NA","NA","Out of scope. See declaration on tuffbau website",50601739400041,"NA","NA",5060173940041,5060173940041,5060173940041]
["Enter product 002"]
["Enter product 003"]
["Enter further items"]